
Packet Tracer – Troubleshoot VTP and DTP

1. Topology



1. Addressing Table

|  |  |  |
| --- | --- | --- |
| Device | IP Address | Subnet Mask |
| PC0 | 172.16.10.1 | 255.255.255.0 |
| PC1 | 172.16.20.1 | 255.255.255.0 |
| PC2 | 172.16.30.1 | 255.255.255.0 |
| PC3 | 172.16.30.2 | 255.255.255.0 |
| PC4 | 172.16.20.2 | 255.255.255.0 |
| PC5 | 172.16.10.2 | 255.255.255.0 |
| S1 | 172.16.99.1 | 255.255.255.0 |
| S2 | 172.16.99.2 | 255.255.255.0 |
| S3 | 172.16.99.3 | 255.255.255.0 |

1. Objectives

Part 1: Troubleshoot DTP

Part 2: Troubleshoot VTP

1. Background / Scenario

In this activity, the switches S2 and S3 are not implementing VTP information. You will verify that DTP and VTP configurations are correctly implemented. When all the issues are resolved, the PCs in the same VLAN will be able to communicate with each other.

1. Troubleshoot DTP

In Part 1, you will troubleshoot the trunk links among the switches. You will verify that permanent trunk links are used between the switches.

* + - 1. Enter **show interfaces trunk** at the privileged EXEC prompt on all the switches to determine the status of the trunk links. How many trunk links are configured currently?

**no trunks links between switches**

Enter **show interfaces g0/1 switchport** at the privileged EXEC prompt on S1. Do the same for g0/2 interface on S1.

What is the operational mode on the GigabitEthernet interfaces on S1? **Static access**

* + - 1. Repeat the commands for g0/1 on S2 and g0/2 on S3.

Correct the trunk links. Record the commands you used to correct the trunking issue.

**On S1: int range g0/1-2**

**Switchport mode trunk**

**On S2: int g0/1**

**Switchport mode trunk**

**On S3 : int g0/2**

**Switchport mode trunk**

* + - 1. Verify the trunk links using the **show** commands.
      2. Show interfaces trunk

1. Troubleshoot VTP
   * 1. Verify VLAN information

Use the **show vlan brief** command on all the switches. Do all the switches have the same number of VLANs? How many does each switch have?

**No. S1 has 10 vlans, s2 and s3 have 7 vlans each.**

* + 1. Verify VTP configurations.

Use the **show vtp status** and **show vtp password** commands on all the switches to verify the VTP status.

Record the VTP status information in the table below.

|  |  |  |  |
| --- | --- | --- | --- |
| Device | Domain Name | Operating Mode | VTP Password |
| S1 |  |  |  |
| S2 |  |  |  |
| S3 | ccna | Transparent | Cisco |

* + 1. Correct the VTP configurations.

Ensure that switch S1 is operating as the VTP server. S2 and S3 should be VTP clients, and receiving VTP updates from S1. The VTP domain should be **CCNA**and the VTP password should be **cisco**. The desired VLANs are already configured on switch S1

Record the commands used to correct the VTP configurations.

**On S1:**

**Vtp mode Server**

**Vtp domain CCNA**

**Vtp password cisco**

**On S2 y S3**

**Vtp mode client**

**Vtp domain CCNA**

**Vtp password cisco**

* + 1. Verify port assignment.

The switchports connecting to the PCs need to be configured in the correct VLANs so the PCs can communicate with each other.

Use the **show vlan brief** command on S2 and S3 to determine if VLANs have been assigned to the switchports. Which VLAN is associated with these switchports? **Just Vlan 1**

|  |  |  |
| --- | --- | --- |
| Ports | Assignments | Network |
| S2 F0/1  S3 F0/8 | VLAN 10 (Staff) | 172.16.10.0/24 |
| S2 F0/9  S3 F0/16 | VLAN 20 (Student) | 172.16.20.0 /24 |
| S2 F0/17  S3 F0/24 | VLAN 30 (Faculty) | 172.16.30.0 /24 |

Using the table above, correct the VLAN assignments on S2 and S3. Record the VLAN assignment configurations below.

* + 1. Verify end to end connectivity.
       1. From PC0 ping PC5.
       2. From PC1 ping PC4.
       3. From PC2 ping PC3.